German Razo

CSCI551

Report

Value of N used: 44083498

Absolute Relative True Error: 4.9344706640471111563e-15

Table of timings for all runs

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Runs** | | |
|  | **1** | **2** | **3** |
| **comm\_sz (number of cores)** |  |  |  |
| **2** | 14.7742 | 14.7787 | 14.7778 |
| **8** | 3.7365 | 3.7128 | 3.7253 |
| **14** | 2.1261 | 2.1856 | 2.1291 |
| **20** | 1.5069 | 1.5085 | 1.5311 |

Speedup for each configuration

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Runs** | | |
|  | 1 | **2** | **3** |
| **comm\_sz (number of cores)** |  |  |  |
| **2** | 1.8329 | 1.8323 | 1.8324 |
| **8** | 7.2473 | 7.2936 | 7.2691 |
| **14** | 12.7366 | 12.3897 | 12.7185 |
| **20** | 17.9703 | 17.9508 | 17.6855 |

Efficiency for each configuration

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Runs** | | |
|  | **1** | **2** | **3** |
| **comm\_sz (number of cores)** |  |  |  |
| **2** | .91645 | .916175 | .9162 |
| **8** | .90592 | .911711 | .9086 |
| **14** | .90976 | .884979 | .9084 |
| **20** | .89851 | .897541 | .8842 |

**Table of minimum times with estimated integral, absolute relative true error,**

**And calculated speedup and efficiency**.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Minimum time** | **Estimated integral** | **ABSTRE** | **Calculated Speedup** | **Efficiency** |
| **2** | 14.774259 | 4.7540192288588e+03 | 5.0344230268089317103e-15 | 1.8329 | .9164 |
| **8** | 3.712802 | 4.7540192288588e+03 | 5.0129379394862973857e-15 | 7.2936 | .9117 |
| **14** | 2.126143 | 4.7540192288588e+03 | 5.0439511959694043240e-15 | 12.7366 | .9097 |
| **20** | 1.506926 | 4.7540192288588e+03 | 5.0396541785048774588e-15 | 17.9703 | .8985 |

Speedup Graph, minimum times

Efficiency Grpah, minimum times

**Discussion of results and conclusion:**

I observed that as number of processes increases, time decreases. In fact, if the size of the processes increases by almost doubling the number of processes, times also decreases by more than half the previous times, for instance, when running the program with 2 cores and 8 cores there’s a huge improvement on times, it is observed that times decrease from 14.772 to 3.7 seconds for minimum times. On the other hand, from 8 to 20 processes there is not a big difference as observed from 2 to 8, and 14 to 20 processes. However, it is still a big improvement that time decrease from 3.73 to 1.5 seconds. The common pattern that it is observed from the timings is the decrease of time as number of processes increases, and this is something that is expected, however, the more processes the less decrease of time is also observed as I mentioned from 2 to 8 and 14 to 20 processes.

To obtain perfect parallelization T1 (time to complete the task on processor) / TP (time for p processors) must equal number of processors and this is rarely achieved and sometimes is not possible to get this linear speedup. Having sad that, the speedups obtained by all the runs were approximate to the number of processors and this is I believe a good result. The number of processes that were the closest to number of processors were 2 and 8, for 2 processes speedup was 1.8, and for 8 processes speedup was 7.2, so this is approximate to number of processors, which is favorable. On the other hand, as number of processors increase, speedup was close, but not as much as less number of processors, so for number of processes 14 and 20, speedup obtained for 14 was 12.73 and for process 20 speedup was 17.97. So, as the number of processes increases, speedup is not approximate to number of processors and the less processes the better speedup was achieved in my program.

When achieving an efficiency of 1 is considered perfect parallelization and is not likely to happen, however, most of the efficiency obtained for each run was close to 1.0, so all the runs that were made by each processor resulted in a good efficiency. As in speedup, the less processors the better efficacy because with two processors an efficiency of .91 was reached and for 20 processors a efficiency of .89 was reach, so efficiency was near linear.

The results of efficiency and speedup are represented on my graphs, and as I mentioned less processors have better results than more processors. Speedup increases and efficiency decreases.

In conclusion, I believe every run achieve a good result on efficiency and speedup, and it is unlikely to achieve perfect speedup and efficiency because of the communication between processes or some portions might not be fully parallelized. However, the results and the graph gave a better representation of how speedup and efficiency is achieved and how the number of processors affect these results.